Steps:

Install Arduino –Arduino Should be running Standard Firmata (Examples library)

Install Node.js

Install Leapmotion With SDK

Run Node Command Prompt from the downloaded folders:

npm install johnny-five

cd to src directory with app2.js

node app2.js

Troubleshooting

If anything else is connected to COM ports, disable them